**K1T605 Series Face Recognition Terminal**

**Release Notes (2018-12-03)**

|  |  |  |
| --- | --- | --- |
| **Device Model:**DS-K1T605EDS-K1T605EFDS-K1T605MDS-K1T605MFDS-K1T605MF-B | Firmware Version | ARM:ACS\_605\_EN\_GM\_V1.1.0\_build181114MCU:ACS\_MCU\_TRIANGLE\_GML\_GM\_V1.0.0\_build180612 |
| iVMS-4200 Client Version | V2.6.10.18 build20181018 |

**Note:** Upgrade both MCU and ARM firmware together to achieve fully upgrade.

**Reason of Upgrade**

Add or modify functions, fix bugs, enhance products quality and meet customers’ requirements.

**Modified Features**

1. Improve live face detection algorithm;
2. Default value for 1:N face recognition change to normal level;
3. Pupillary distance requirement for face enrollment (local and photo import) adjust to 60;
4. Support output card number by 485.

**Customer Impact and Recommended Action**

This new firmware upgrade is to improve product performance, and will take effect automatically after upgrading from previous versions. We’d like to inform you the above changes. Also, we are sorry for any possible inconvenience of use-habit changes caused by this action.

For questions or concerns, please contact our local technical support team.

Note:

* Hikvision has all rights to alter, modify and cancel this notice.
* Hikvision doesn’t give any guarantee for old models’ stock.
* Hikvision is not liable for any typing or printing errors.
* For special model’s change details, please contact our local technical support team.

Hikvision Digital Technology CO., Ltd.

No. 555 Qianmo Road, Binjiang District, Hangzhou 310052, China

Tel: +86-571-8807-5998

FAX: +86-571-8993-5635

Email: support@hikvision.com