**DS-K5603(T)-Z Face Recognition Terminal V1.1build181112 Release Notes**

|  |  |  |
| --- | --- | --- |
| **Device Model:**DS-K5603-ZDS-K5603T-Z | Firmware Version | ARM: ACS\_5603\_15\_AI0\_CN\_GM\_V1.1.0\_build181112MCU: ACS\_DS-K560X-NORF\_GML\_GM\_V1.0.0\_build181025 |
| SDK Version | HCNetSDKV5.3.6.15\_build20180705\_win32 |
| 4200 Version | V2.6.10.14 build20180824 |
| Ehome Version | EhomeSDK\_V1.2.1.13\_build20180803\_win32 |

**Reason of Upgrade**

Add or modify functions, fix bugs, enhance products quality and meet customers’ requirements.

**Modified Features**

1. Minimum pupillary distance for face enrollment (local and photo import) decreases from 60 to 40 to make face enrollment process much easier.
2. Improve live face detection algorithm.
3. Auto adjust white light function is disabled by default, and white light brightness default value changes to 40.
4. When applying face data and permission to device, device can keep in normal working mode. That means you can get permission and go through even during device permission applying period.

**Customer Impact and Recommended Action**

This new firmware upgrade is to improve product performance, and will take effect automatically after upgrading from previous versions. We’d like to inform you the above changes. Also, we are sorry for any possible inconvenience of use-habit changes caused by this action.

For questions or concerns, please contact our local technical support team.

Note:

* Hikvision has all rights to alter, modify and cancel this notice.
* Hikvision doesn’t give any guarantee for old models’ stock.
* Hikvision is not liable for any typing or printing errors.
* For special model’s change details, please contact our local technical support team.

Hikvision Digital Technology CO., Ltd.

No. 555 Qianmo Road, Binjiang District, Hangzhou 310052, China

Tel: +86-571-8807-5998

FAX: +86-571-8993-5635

Email: support@hikvision.com