**How to Make Schedule Backup History Video in IVMS-4200**

**Note:** As we all know, we can add Hybird SAN into IVMS-4200 and configure recording schedule for each camera. This manual will show you how to do it and points for attention. The version of IVMS-4200 is v2.7.2.4 which supports to make schedule backup history video template.


*IVMS-4200 download Link: https://www.hikvision.com/en/Support/Downloads/Client-Software*

# Steps

1. *You need to insert the hard driver before configuring device. And the disk should be installed in right position as follow pictures.*


# Wrong Installation Correct Installation

1. *The status of disk is* ***unauthorized*** *when you insert new disk into device.so you need to check or detect it. The status of disk will be* ***Normal*** *after checking or* detectin







1. *Add Hybird SAN device into IVMS-4200 in device management interface. You need to input IP address, user name and password.*




1. *Click* ***Remote Configuration****, And you will enter configuration interface. In the storage interface, Click*

***General****, and just click* ***One-touch Config*** *which will start to automatically configure Hybird SAN service. When the one-touch config finish, the status of hybrid san will be Working .*

**









1. *After one-touch configuration, you can start to make recording schedule in* ***storage schedule*** *interface.*


Choose the camera in left bar which you want to make recording schedule. And then choose **storage server**

and **related HDD**. Finally, The recording schedule should be empty template.


****

1. *After configuring empty template schedule. Click* ***Remote configuration*** *in the device management. *
2. *And Click* ***Uploading Historical Record in Event option,*** *you can set which certain period of video you want to backup. In this case, make a backup schedule for this camera is that from 8 am to 6 pm. But you also can make an all-day template for it. So it depends on project requirements.*







1. *Click* ***Uploading Execution Plan Configuration,*** *you can set when you want to start to backup video from NVR/DVR/IPC. In this case, make execution plan from 0 am to 8 am and from 6 pm from to 24 pm. You can set all-day template for it as well if necessary.*



1. *Then login hybrid san system to check the status of upload.*





**First Choice for Security Professionals**

***HIKVISION* Technical Support**