
**How to Make Recording Schedule in IVMS-4200**

***Note:*** *As we all know, we can add Hybird SAN into IVMS-4200 and configure recording schedule for each camera. This manual will show you how to do it and points for attention. The version of IVMS-4200 is v2.7.0.10 which supports to make schedule backup history video template.*

*IVMS-4200 download Link: http://www.hikvision.com/en/Tools\_84.html*

**

***Steps***

1. *You need to insert the hard driver before configuring device. And the disk should be installed in right position as follow pictures.*


******




***Wrong Installation Correct Installation***


1. *The status of disk is* ***unauthorized*** *when you insert new disk into device.so you need to check or detect it.*

*The status of disk will be* ***Normal*** *after checking or detecting.*


**


**

1. *Add Hybird SAN device into IVMS-4200 in device management interface. The device type belongs to* ***storage server****. You need to input IP address, user name and password.*

**


1. *Click* ***Remote Configuration****, And you will enter configuration interface. In the storage interface, Click* ***General****, and just click* ***One-touch Config*** *which will start to automatically configure Hybird SAN service.*

**

**

1. *After one-touch configuration, you can start to make recording schedule in* ***storage schedule*** *interface.*

*Choose the camera in left bar which you want to make recording schedule. And then choose* ***storage server*** *and* ***related HDD****. Finally, Configure record schedule template for camera and click* ***save*** *button on right top.*

****

**First Choice for Security Professionals**

***HIKVISION* Technical Support**