
**How to add IP SAN storage in windows storage server**


***Note:*** *This file will tell you how to add IP SAN storage in storage server.*

***Steps***


1. *Click LUN in left bar and enter the LUN interface. Click Create button, input LUN name and LUN size.*

******


1. *Right click the* ***SAN Management*** *in the left bar. Click* *iSCSI and enter the iSCSI interface. And then click* ***Enable iSCSI,*** *input the Client IP which is the IP address of storage server.*

**


1. *Input**iSCSI in the windows and click the iSCSI initiator.*





1. *Click the Discover* ***portal button*** *in the iscsi initiator Properties, and input the IP address of IP SAN, Click OK.*




1. *You can see the targets of IP SAN in the target portals list.*




1. *Click the* ***Targets*** *in the top bar. You can see the Discovered targets and click the* ***connect*** *, check the* ***connected*** *status.*

 a



1. *Click the* ***Disk management*** *in the Storage and you will find a new disk, and click* ***OK.***




1. *You will see the* ***unallocated*** *disk in the Disk bar, Right click the* ***unallocated***




1. *Click the* ***Next*** *button in the new simple volume wizard until final step.*



1. *You can see the status of disk is* ***formatting,*** *you can check the disk in the hard disk drivers after formatting finished.*





**First Choice for Security Professionals**

***HIKVISION* Technical Support**