
**How to use DS-KC001**

**Step 1.**


Active the device

(the password must same as Temperature MinMoe Terminal)




**Step 2.**


If you don’t connect the network cable, the Wi-Fi configuration interface will pop up automatically.



**Step 3.**


If you are using a wired network, you can obtain an available IP address by turning on DHCP\





**Step 4.**

Select the Temperature MinMoe Terminal to be bound



**Note.**

The ‘temperature measurement only’ mode is a thermal imaging picture; the visible light pictures will be taken after authentication.

(It depends on the version of MinMoe Terminal)

**See Far Go Farther**

***HIK*VISION Technical Support**