**Main Control Board V1.0.3\_** **build20220121**

**Release Note (2022-02-11)**

|  |  |  |
| --- | --- | --- |
| **Device Model:**DS-K3M200-B501SX/B601SX/B801SX/Y501SX/ B802X | Firmware Version | ACS\_DS-K3M200\_ST0\_GML\_GM\_V1.0.3\_build20220121 |

**Reason for update:**

【new features】

None

【Improved function】

1. Fix the problem of missing card number during the defragmentation process after the card is fully loaded and downloaded.

2. Fix device IP exception when the MCU closes the TCP connection.

3. Fix the occasional time becomes 2036 problem in the NTP calibration time.

【Remaining problem】

None

***Remarks:***

* Hikvision reserves the right to change, alter or withdraw the above notification without prior notice.
* Product design and specifications are subject to change without prior notice.
* The Hikvision firmware may contain errors known as errata which may cause the product to deviate from published specifications. Current characterized errata are available on request.
* Hikvision is not liable for any typing or printing errors.

Hikvision Digital Technology CO., Ltd.

No. 555 Qianmo Road, Binjiang District, Hangzhou 310051, China

Tel: +86-571-8807-5998

FAX: +86-571-8993-5635

Email: overseabusiness@hikvision.com