**How to Make Recording Schedule in HikCentral**

***Note:*** *As we all know, we can add Hybird SAN into HikCentral and configure recording schedule for each camera. This manual will show you how to do it and points for attention.*

***Steps***

1. *You need to insert the hard driver before configuring device. And the disk should be installed in right position as follow pictures.*


******




***Wrong Installation Correct Installation***


1. *The status of disk is* ***unauthorized*** *when you insert new disk into device.so you need to check or detect it.*

*The status of disk will be* ***Normal*** *after checking or detecting.*


**


**

1. *Add Hybird SAN device into HikCentral in device management interface. The device type belongs to* ***Recording server****. You need to input IP address, user name and password. Then click Add.*




1. *Click* ***One-touch Config*** *,there is a pop-up window to select the type of RAID, normally is RAID 5, then click OK, which will start to automatically configure Hybird SAN service,*






1. *After one-touch configuration, you can start to make recording schedule in* ***Logical view*** *interface.*

*Choose the group in left bar which you want to make recording schedule. And then click the camera. choose* ***storage server*** *and* ***related volume****. Finally, Configure record schedule template for camera and click* ***save*** *button .*





**First Choice for Security Professionals**

***HIKVISION* Technical Support**